|  |  |
| --- | --- |
| EAN 5901804191497 | CB NUMBER T2202 |
| Vendor Art. Nr 1804191497 |  |

HARLEY

# Main description

Harley is one of the most original radiator designs available on the market. The shape of this radiator is based on an intriguing geometric pattern with harmoniously arranged pairs of profiles. Harley can provide an attractive focal point in modern living rooms, halls and recreational spaces.

# Key points


* Unique profile arrangement
* Harmonious proportions and style
* Can add a new dimension to your interior
* Adheres very close to the wall

# Features and benefits

* Highest quality low carbon steel ensuring product longevity
* Excellent heat output
* Every rail 100% leak tested
* Oxsilan® passive rust protection process
* High quality double layer powder coating
* Up to 8 Year Guarantee
* Increased resistance to chemicals, temperature variations and mechanical damage
* Easy installation (solid wall fixing kit included)
* Made to EN 10305-5
* Easy cleaning and maintenance

# Specifications

|  |  |
| --- | --- |
| Height (mm): | 1400 |
| Width (mm): | 530 |
| Depth (mm): | 50 |
| Colour: | Heban |
| Heat output (W): | 523 |
| Heat output (BTUs): | 1785 |
| Connection type: | SX |
| Connection spacing (mm): | 500 |
| Wall to centre of inlet (mm): | 62-70 |
| Operating pressure (MPa): | 0.8 |
| Maximum operating temperature (°C): | 95 |
| Material: | Carbon steel |
| Surface finish: | Powder coating |
| Weight (kg): | 10.7 |

Connection diagram